FILE_TYPE = MULTI_PHYS_TABLE;

PART 'CD4050BE'
CLASS = IC
{========================================================================================}
:"MANUFACTURER_NAME", "MANUFACTURER_PART_NUMBER"= "PART_NUMBER", "JEDEC_TYPE", "PACK_TYPE", "MOUSER_PART_NUMBER", "MOUSER_PRICE/STOCK", "ARROW_PART_NUMBER", "ARROW_PRICE/STOCK", "DESCRIPTION", "DATASHEET", "HEIGHT";
{========================================================================================}
 "Texas Instruments", "CD4050BE" (!) = "", "DIP794W53P254L1930H508Q16N", "Dual-In-Line Packages", "595-CD4050BE", "https://www.mouser.co.uk/ProductDetail/Texas-Instruments/CD4050BE?qs=j%2FZo4ajzVJLKLpJvKsajlg%3D%3D", "CD4050BE", "https://www.arrow.com/en/products/cd4050be/texas-instruments?utm_currency=USD&region=nac", "CD4050BE, Hex Inverter Buffer, Converter, 26mA -0.5  20 V 16-Pin PDIP", "http://www.ti.com/lit/ds/symlink/cd4049ub.pdf", "5.08 mm"
END_PART

END.
