(part "S41-2V"
    (packageRef "S412V")
    (interface
        (port "1" (symbPinId 1) (portName "COIL+") (portType INOUT))
        (port "2" (symbPinId 2) (portName "NO_1") (portType INOUT))
        (port "3" (symbPinId 3) (portName "COM_1") (portType INOUT))
        (port "4" (symbPinId 4) (portName "COM_2") (portType INOUT))
        (port "5" (symbPinId 5) (portName "NO_2") (portType INOUT))
        (port "6" (symbPinId 6) (portName "NO_CONNECTION_1") (portType INOUT))
        (port "7" (symbPinId 7) (portName "NO_CONNECTION_2") (portType INOUT))
        (port "8" (symbPinId 8) (portName "NO_3") (portType INOUT))
        (port "9" (symbPinId 9) (portName "COM_3") (portType INOUT))
        (port "10" (symbPinId 10) (portName "COM_4") (portType INOUT))
        (port "11" (symbPinId 11) (portName "NO_4") (portType INOUT))
        (port "12" (symbPinId 12) (portName "COIL-") (portType INOUT))
    )
    (partClass UNDEF)
    (useInSchema Y)
    (useInLayout Y)
    (inPartsList Y)
    (partType NORMAL)
    (placeRestriction FREE)
    (property "compKind" "161")
    (property "Manufacturer_Name" "Panasonic")
    (property "Manufacturer_Part_Number" "S41-2V")
    (property "Mouser_Part_Number" "")
    (property "Mouser_Price/Stock" "")
    (property "Arrow_Part_Number" "")
    (property "Arrow_Price/Stock" "")
    (property "Description" "General Purpose Relays,Wide switching range From 100A 100 mV DC to 4 A 250 V AC")
    (property "Datasheet_Link" "https://www.farnell.com/datasheets/16770.pdf")
    (property "symbolName1" "S41-2V")
)
